|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Contractor Company’s Ladder: | |  | | | | |
| Contractor Competent Person: |  | | Sign |  | Date: |  |

**Inspection Items**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **No** | **Item** | **Good Condition** | **Needs**  **Repair** | **N/A** |
| 1. | **Label:** |  |  |  |
| a. | Ladder is labelled or marked with its load and duty rating (1A or greater) |  |  |  |
| 2. | **Ladder Parts:** |  |  |  |
| a. | All parts are in place and free of defects (cracks, dents, bends, splits, sharp edges, corrosion, rust, exposed fiberglass, rot, decay, or excessive wear) |  |  |  |
| b. | Rungs, steps, and side rails are connected securely |  |  |  |
| c. | Bolts, rivets, nails, and screws are secure |  |  |  |
| d. | Moving parts move freely without binding or too much play |  |  |  |
| e. | Safety shoes or padded feet are in good repair and clean - not excessively worn |  |  |  |
| 3. | **Extension Ladders:** |  |  |  |
| a. | Metal bearings in locks, wheels, and pulleys are lubricated |  |  |  |
| b. | Locks or latching mechanisms are not missing, broken, or loose |  |  |  |
| c. | Locking guides or brackets engage properly |  |  |  |
| d. | Rope tracks properly in the pulley |  |  |  |
| e. | Ropes are not frayed, cut, badly worn, burned, or showing mildew or rot |  |  |  |
| f. | Ropes are free of tangles |  |  |  |
| 4. | **Stepladders**: |  |  |  |
| a. | Spreader bars are tight and have all rivets |  |  |  |
| b. | Spreader bars open fully and lock |  |  |  |

|  |
| --- |
| **Remarks:** |
|  |
|  |
|  |
|  |