|  |  |  |  |
| --- | --- | --- | --- |
|  Name: |  | Instructor: |  |
| Company: |  | Project Name: |  |
| 1st day on job (date): |  | Project No.: |  |
| Title: |  | Date: |  |
| Sticker No.: |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  | **YES** | **NO** | **NA** |
| **PPE** |  |  |  |
| Inspect before use |  |  |  |
| Hard hat, safety glasses & vest must be worn |  |  |  |
| Long pants, shirt w/ 4” sleeves and hard soled work boots are required |  |  |  |
| Hearing protection |  |  |  |
| Eye & face protection  |  |  |  |
| Gloves (as required) |  |  |  |
| Respiratory protection (as required) |  |  |  |
| Reflective vest or high visibility clothing worn |  |  |  |
| **HOUSEKEEPING** |  |  |  |
| Housekeeping required daily |  |  |  |
| **EMERGENCY ACTION PLAN** |  |  |  |
| Accident/Emergency reporting procedure |  |  |  |
| Location of emergency phone numbers |  |  |  |
| Evacuation routes and procedure |  |  |  |
| **HAZ COMM PLAN** |  |  |  |
| Location of material safety data sheets |  |  |  |
| Review of chemicals on the jobsite |  |  |  |
| Location of First Aid Kits |  |  |  |
| **FIRE PROTECTION** |  |  |  |
| Location of fire extinguishers |  |  |  |
| Hot work control & permit requirements |  |  |  |
| Fire extinguishers training PASS |  |  |  |
| Storage & Handling of flammable liquids |  |  |  |
| Storage & handling of compressed gas cylinders |  |  |  |
| **LADDERS** |  |  |  |
| Weight capacity label required on ladders  |  |  |  |
| Ladders must be secured top and bottom |  |  |  |
| Ladders must extend 3’ above landing surface  |  |  |  |
| Do not stand on the top step of any ladder |  |  |  |
| No Green (Verde) ladders allowed on site (1A or greater) |  |  |  |
| **ELECTRICAL** |  |  |  |
| All tools, cords, and welding leads must be free of damage |  |  |  |
| No tape on cords, ground prong intact |  |  |  |
| GFCl protection required always |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  | **YES** | **NO** | **NA** |
| **SCAFFOLDS (>6’)** |  |  |  |
| Guardrails required if platform is 6’ or higher |  |  |  |
| Platform must be fully planked |  |  |  |
| Ladder or stair access must be used |  |  |  |
| Do not move rolling scaffold while occupied |  |  |  |
| **FALL PROTECTION SYSTEMS** |  |  |  |
| Inspect PFAS |  |  |  |
| Review 6’ fall protection rule |  |  |  |
| Proper use of Harness, Lanyard, anchorage |  |  |  |
| Do not remove guardrails/hole covers |  |  |  |
| Do not lean on guardrails  |  |  |  |
| All holes 2” and larger must be covered |  |  |  |
| **TOOL & EQUIPMENT SAFETY** |  |  |  |
| Seat belts must be worn always |  |  |  |
| Rigging must be inspected daily |  |  |  |
| Guards must be used |  |  |  |
| Hoisting (duct jack) equipment inspected |  |  |  |
| Back up alarms or spotter required |  |  |  |
| Fall Protection required when working on aerial/boom lift |  |  |  |
| Forklift operators must be trained & licensed |  |  |  |
| Crane operators licensed  |  |  |  |
| **TRENCHING/EXCAVATION** |  |  |  |
| Never enter any trench or excavation until authorized by the competent person |  |  |  |
| Protective systems (sloping, shoring, etc.) required when over 5’ deep |  |  |  |
| Ladders/ ramp access required when >4’ |  |  |  |
| **MISCELLANEOUS** |  |  |  |
| Substance Abuse Policy & Post Accident Drug Testing |  |  |  |
| Review of Three Step Disciplinary Policy |  |  |  |
| Aerial lift operators trained by employer |  |  |  |
| Procedure to Report Unsafe Conditions |  |  |  |
| Identify of First Aid trained personnel |  |  |  |
| Site Specific Safety Rules & Procedures |  |  |  |
| Weapons (fire arms) are prohibited |  |  |  |
| No listening to music on site |  |  |  |
| Repeated safety violations grounds for removal |  |  |  |
| Exposed to unprotected falls grounds for removal |  |  |  |
| Sexual harassment will be grounds for removal |  |  |  |
| I have seen and understand this safety video |  |  |  |

##